|  |
| --- |
| webwxgetmsgimg (7).jpeg |

|  |
| --- |
| Technical Specification |
|  |

|  |
| --- |
| O-RAN Work Group 3 (Near-RT RIC and E2 Interface)  E2 Service Model (E2SM) |

|  |
| --- |
|  |
| Copyright © 2024 by the O-RAN ALLIANCE e.V.  The copying or incorporation into any other work of part or all of the material available in this specification in any form without the prior written permission of O-RAN ALLIANCE e.V. is prohibited, save that you may print or download extracts of the material of this specification for your personal use, or copy the material of this specification for the purpose of sending to individual third parties for their information provided that you acknowledge O-RAN ALLIANCE as the source of the material and that you inform the third party that these conditions apply to them and that they must comply with them.  O-RAN ALLIANCE e.V., Buschkauler Weg 27, 53347 Alfter, Germany  Register of Associations, Bonn VR 11238, VAT ID DE321720189 |

"© 2019. 3GPP™ TSs and TRs are the property of ARIB, ATIS, CCSA, ETSI, TSDSI, TTA and TTC who jointly own the copyright in them. They are subject to further modifications and are therefore provided to you "as is" for information purposes only. Further use is strictly prohibited."

"© 2020. 3GPP™ TSs and TRs are the property of ARIB, ATIS, CCSA, ETSI, TSDSI, TTA and TTC who jointly own the copyright in them. They are subject to further modifications and are therefore provided to you "as is" for information purposes only. Further use is strictly prohibited."

"© 2021. 3GPP™ TSs and TRs are the property of ARIB, ATIS, CCSA, ETSI, TSDSI, TTA and TTC who jointly own the copyright in them. They are subject to further modifications and are therefore provided to you "as is" for information purposes only. Further use is strictly prohibited."

Contents

List of tables 4

Foreword 5

Modal verbs terminology 5

1 Scope 6

2 References 6

2.1 Normative references 6

2.2 Informative references 7

3 Definition of terms, symbols and abbreviations 7

3.1 Terms 7

3.2 Symbols 7

3.3 Abbreviations 7

4 General 8

4.1 Procedure Specification Principles 8

4.2 Forwards and Backwards Compatibility 8

4.3 Specification Notations 8

5 E2SM services 8

6 Common Elements for E2SM Service Models 10

6.1 General 10

6.2 Information Element definitions 10

6.2.1 General 10

6.2.2 E2SM common IEs 10

6.2.3 3GPP derived IEs 17

6.3 Information Element Abstract Syntax (with ASN.1) 27

6.3.1 General 27

6.3.2 Information Element definitions 27

6.3.3 Message transfer syntax 35

Annex (informative): Change History 36

# List of tables

[Table 5-1: Relationship between RAN Function specific E2AP Information elements and E2AP Procedures 8](#_Toc151468184)

[Table 5-2: O-RAN specified E2 Service Models and related OIDs 9](#_Toc151468185)

# Foreword

This Technical Specification (TS) has been produced by WG3 of the O-RAN Alliance.

The content of the present document is subject to continuing work within O-RAN and may change following formal O-RAN approval. Should the O-RAN Alliance modify the contents of the present document, it will be re-released by O-RAN with an identifying change of version date and an increase in version number as follows:

version xx.yy.zz

where:

xx: the first digit-group is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc. (the initial approved document will have xx=01). Always 2 digits with leading zero if needed.

yy: the second digit-group is incremented when editorial only changes have been incorporated in the document. Always 2 digits with leading zero if needed.

zz: the third digit-group included only in working versions of the document indicating incremental changes during the editing process. External versions never include the third digit-group. Always 2 digits with leading zero if needed.

# Modal verbs terminology

In the present document "**shall**", "**shall not**", "**should**", "**should not**", "**may**", "**need not**", "**will**", "**will not**", "**can**" and "**cannot**" are to be interpreted as described in clause 3.2 of the O-RAN Drafting Rules (Verbal forms for the expression of provisions).

"**must**" and "**must not**" are **NOT** allowed in O-RAN deliverables except when used in direct citation.

# 1 Scope

The present document describes the O-RAN specified RAN Function-specific Service Models supported over E2 (E2SM) and specifies the common elements for use in E2 service models.

# 2 References

## 2.1 Normative references

References are either specific (identified by date of publication and/or edition number or version number) or non‑specific. For specific references, only the cited version applies. For non-specific references, the latest version of the referenced document (including any amendments) applies.

NOTE 1: In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document in 3GPP Release 17.

NOTE 2: While any hyperlinks included in this clause were valid at the time of publication, O-RAN cannot guarantee their long-term validity.

The following referenced documents are necessary for the application of the present document.

[1] 3GPP TR 21.905: “Vocabulary for 3GPP Specifications”.

[2] O-RAN.WG3.E2GAP, “O-RAN Working Group 3, Near-Real-time RAN Intelligent Controller, Architecture & E2 General Aspects and Principles (E2GAP)”

[3] O-RAN.WG3.E2AP, “O-RAN Working Group 3, Near-Real-time RAN Intelligent Controller, E2 Application Protocol (E2AP)”.

[4] ORAN Working Group 3, Near-Real-time RAN Intelligent Controller, E2 Service Model, Network Interface (E2SM-NI).

[5] ORAN WG3, O-RAN Working Group 3, Near-Real-time RAN Intelligent Controller, E2 Service Model, KPI Monitor (E2SM-KPM).

[6] 3GPP TS 38.413: “NG-RAN; NG Application Protocol (NGAP)”.

[7] 3GPP TS 38.423: “NG-RAN; Xn Application Protocol (XnAP)”.

[8] 3GPP TS 38.473: “NG-RAN; F1 Application Protocol (F1AP)”.

[9] 3GPP TS 37.483: “E1 Application Protocol (E1AP)”.

[10] 3GPP TS 36.413: “E-UTRAN; S1 Application Protocol (S1AP)”

[11] 3GPP TS 36.423: “E-UTRAN; X2 Application Protocol (X2AP)”.

[12] 3GPP TS 37.473: “W1 interface; Application Protocol (W1AP)”.

[13] 3GPP TR 25.921: “Guidelines and principles for protocol description and error handling”.

[14] 3GPP TS 36.331: “E-UTRA; Radio Resource Control (RRC) Protocol Specification”.

[15] 3GPP TS 38.331: “NR; Radio Resource Control (RRC) Protocol Specification”.

[16] ITU-T Recommendation X.680 (07/2002): "Information technology – Abstract Syntax Notation One (ASN.1): Specification of basic notation".

[17] ITU-T Recommendation X.681 (07/2002): "Information technology – Abstract Syntax Notation One (ASN.1): Information object specification".

[18] O-RAN.WG1.OAD, “O-RAN Architecture Description”.

## 2.2 Informative references

References are either specific (identified by date of publication and/or edition number or version number) or non‑specific. For specific references, only the cited version applies. For non-specific references, the latest version of the referenced document (including any amendments) applies.

NOTE: While any hyperlinks included in this clause were valid at the time of publication, O-RAN cannot guarantee their long-term validity.

The following referenced documents are not necessary for the application of the present document, but they assist the user with regard to a particular subject area.

Not applicable.

# 3 Definition of terms, symbols and abbreviations

## 3.1 Terms

For the purposes of the present document, the terms given in 3GPP TR 23.905 [1], O-RAN WG3.E2GAP [2] and O-RAN WG1.OAD [18] and the following apply:

**Format Type**: The identifier used to nominate a specific formatting approach used to encode one of the E2AP IEs defined in this E2SM.

**RAN Function specific E2AP Information Element**: An E2SM specific implementation of a container used to carry an E2AP [3] defined E2SM specific IE.

**Style Type**: The identifier used to nominate a specific approach or Style used to expose a given RIC Service (REPORT, INSERT, CONTROL and POLICY).

## 3.2 Symbols

For the purposes of the present document, the symbols [given in [i.1] and the following] apply:

Void

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 23.905 [1], O-RAN WG3.E2GAP [2] and O-RAN WG1.OAD [18] and the following apply:

Void

# 4 General

## 4.1 Procedure Specification Principles

The procedure specification principles defined in E2AP [3] clause 4 shall apply.

## 4.2 Forwards and Backwards Compatibility

The forwards and backwards compatibility of the E2 interface uses the forward and backwards compatibility compatibilities offered by the E2AP [3] protocol.

## 4.3 Specification Notations

For the purposes of the present document, the following notations apply:

IE When referring to an information element (IE) in the specification the *Information Element Name* is written with the first letters in each word in upper case characters and all letters in Italic font followed by the abbreviation "IE", e.g. *E-RAB ID* IE.

Value of an IE When referring to the value of an information element (IE) in the specification the "Value" is written as it is specified in the specification enclosed by quotation marks, e.g. "Value".

# 5 E2SM services

As defined in E2 General Aspects and Principles [2], a given RAN Function offers a set of services to be exposed over the E2 (REPORT, INSERT, CONTROL, POLICY and/or QUERY) using E2AP [3] defined procedures. Each of the E2AP Procedures listed in table 5-1 contains specific E2 Node RAN Function dependent Information Elements (IEs) which shall be defined by a specific E2SM.

Table 5-1: Relationship between RAN Function specific E2AP Information elements and E2AP Procedures

|  |  |  |  |
| --- | --- | --- | --- |
| RAN Function specific E2AP Information Elements | E2AP Information Element reference | Related E2AP Procedures | |
| *RIC Event Trigger Definition* IE | E2AP [3] clause 9.2.9 | RIC Subscription  RIC Subscription Modification |
| *RIC Action Definition* IE | E2AP [3] clause 9.2.12 | RIC Subscription  RIC Subscription Modification |
| *RIC Indication Header* IE | E2AP [3] clause 9.2.17 | RIC Indication |
| *RIC Indication Message* IE | E2AP [3] clause 9.2.16 | RIC Indication |
| *RIC Call Process ID* IE | E2AP [3] clause 9.2.18 | RIC Indication  RIC Control |
| *RIC Control Header* IE | E2AP [3] clause 9.2.20 | RIC Control |
| *RIC Control Message* IE | E2AP [3] clause 9.2.19 | RIC Control |
| *RIC Control Outcome* IE | E2AP [3] clause 9.2.25 | RIC Control |
| *RIC Query Header* IE | E2AP [3] clause 9.2.36 | RIC Query |
| *RIC Query Definition* IE | E2AP [3] clause 9.2.37 | RIC Query |
| *RIC Query Outcome* IE | E2AP [3] clause 9.2.38 | RIC Query |
| *RAN Function Definition* IE | E2AP [3] clause 9.2.23 | E2 Setup  RIC Service Update |

All of these RAN Function specific E2AP IEs are defined in E2AP [3] as “OCTET STRING”.

The purpose of the E2SM series of specifications is to define the approach that a given RAN Function specific E2 Service Model shall use to define the contents of these fields.

The supported O-RAN specified E2 Service Models are presented in table 5-2.

Table 5-2: O-RAN specified E2 Service Models and related OIDs

|  |  |  |  |
| --- | --- | --- | --- |
| E2SM short name | OID | Syntax language | Scope |
| E2SM-NI | iso(1) identified-organization(3) dod(6) internet(1) private(4) enterprise(1) oran(53148) e2(1) version1 (1) e2sm(2) e2sm-NI-IEs (1) | ASN.1 | RAN Function NI “Network Interface” performs the following functionalities:  - Exposure of Network Interfaces  - Modification of both incoming and outgoing network interface message contents  - Execution of policies that may result in change of network behavior |
| E2SM-KPM version1 | iso(1) identified-organization(3) dod(6) internet(1) private(4) enterprise(1) oran(53148) e2(1) version1 (1) e2sm(2) e2sm-KPM-IEs (2) | ASN.1 | RAN function KPM “KPM Monitor” performs the following functionalities:  - Exposure of O-DU’s cell related performance IEs through periodic KPM Report.  - Exposure of O-CU-CP’s cell/UE related performance IEs through periodic KPM Report.  - Exposure of O-CU-UP’s bearer related performance IEs through periodic KPM Report |
| E2SM-KPM version2 | iso(1) identified-organization(3) dod(6) internet(1) private(4) enterprise(1) oran(53148) e2(1) version2 (2) e2sm(2) e2sm-KPM-IEs (2) | ASN.1 | RAN function KPM “KPM Monitor” performs the following functionalities:  - Exposure of available measurements from O-DU, O-CU-CP, and/or O-CU-UP via the RAN Function Definition IE.  - Periodic reporting of measurements subscribed from Near-RT RIC. |
| E2SM-RC | iso(1) identified-organization(3) dod(6) internet(1) private(4) enterprise(1) oran(53148) e2(1) version1 (1) e2sm(2) e2sm-RC-IEs (3) | ASN.1 | RAN function RC “RAN Control” performs the following functionalities:  - Exposure of RAN control and UE context related information.  - Modification and initiation of RAN control related call processes and messages  - Execution of policies that may result in change of RAN control behavior |
| E2SM-CCC | iso(1) identified-organization(3) dod(6) internet(1) private(4) enterprise(1) oran(53148) e2(1) version1 (1) e2sm(2) e2sm-CCC-IEs (4) | JSON | RAN function CCC “Cell Configuration and Control” performs the following functionalities:  - Exposure of node level and cell level configuration information  - Initiate control and/or configuration of node level and cell level parameters |

# 6 Common Elements for E2SM Service Models

## 6.1 General

Sub clause 6.2 presents the individual information elements that may be adopted by any specific E2SM including the specifications listed in table 5-1. Sub clause 6.3 provides the corresponding ASN.1 definition of each information element, this module may be associated with the ASN.1 definitions in a specific E2SM specification using the ASN.1 "Import" instruction.

The following attributes are used for the tabular description of the messages and information elements:

NOTE: The messages have been defined in accordance to the guidelines specified in 3GPP TR 25.921 [13].

## 6.2 Information Element definitions

### 6.2.1 General

When specifying information elements which are to be represented by bit strings, if not otherwise specifically stated in the semantics description of the concerned IE or elsewhere, the following principle applies with regards to the ordering of bits:

- The first bit (leftmost bit) contains the most significant bit (MSB);

- The last bit (rightmost bit) contains the least significant bit (LSB);

- When importing bit strings from other specifications, the first bit of the bit string contains the first bit of the concerned information.

### 6.2.2 E2SM common IEs

#### 6.2.2.1 RAN Function Name

This IE defines the name of a given *RAN Function Name* IE as a structured data.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| RAN Function Short Name | M |  | PrintableString(SIZE(1..150,...)) | Suitable unique short name |
| RAN Function Service Model OID | M |  | PrintableString(SIZE(1..1000,...)) | Object Identifier of this specific E2SM. Formatted as per OID |
| RAN Function Description | M |  | PrintableString(SIZE(1..150,...)) | Suitable text describing scope of E2SM |
| RAN Function Instance | O |  | INTEGER | Suggested when E2 Node declares multiple RAN Function ID supporting the same E2SM specification |

#### 6.2.2.2 RIC Style Type

This IE defines the identifier of a given RIC Style.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| RIC Style Type | M |  | INTEGER |  |

#### 6.2.2.3 RIC Style Name

This IE defines the name of a given RIC Style.

The same E2SM may support more than one Style for each RIC Service.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| RIC Style Name | M |  | PrintableString(SIZE(1..150,...)) |  |

#### 6.2.2.4 RIC Format Type

This IE defines the identifier of a given RIC Format.

The same E2SM may support more than one encoding Formats for each E2AP IE and each E2AP IE message encoding Format may be used by one or more RIC Service Styles.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| RIC Format Type | M |  | INTEGER |  |

#### 6.2.2.5 Cell Global ID

This IE is used to globally identify a cell in an E2 Node. The IE is derived from TS 38.423 [7] clause 9.2.3.25 "Target Cell Global ID".

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| CHOICE *RAT type* | M |  |  |  |
| *>NR* |  |  |  |  |
| >>NR CGI | M |  | 6.2.3.7 |  |
| *>E-UTRA* |  |  |  |  |
| >>E-UTRA CGI | M |  | 6.2.3.11 |  |

#### 6.2.2.6 UE ID

This IE contains the O-RAN agreed UE ID data structure to be used on E2 interface.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| --- | --- | --- | --- | --- |
| CHOICE *UEID case* | M |  |  |  |
| *>gNB* |  |  |  | E2 Node of type gNB when connected to 5GC |
| >>AMF UE NGAP ID | M |  | 6.2.3.16 |  |
| >>GUAMI | M |  | 6.2.3.17 |  |
| >>gNB-CU UE F1AP ID List | C-ifCUDUseparated |  |  | More than 1 F1AP ID shall be reported by E2 Node only when NR-DC is established. |
| >>>gNB-CU UE F1AP ID Item |  | *1 .. <maxF1APId>* |  |  |
| >>>>gNB-CU UE F1AP ID | M |  | 6.2.3.21 |  |
| >>gNB-CU-CP UE E1AP ID List | C-ifCPUPseparated |  |  |  |
| >>>gNB-CU-CP UE E1AP ID Item |  | *1 .. <maxE1APId>* |  |  |
| >>>>gNB-CU-CP UE E1AP ID | M |  | 6.2.3.20 |  |
| >>RAN UE ID | O |  | 6.2.3.25 |  |
| >>M-NG-RAN node UE XnAP ID | C-ifDCSetup |  | 6.2.3.19 | To be reported by both MN and SN |
| >>Global gNB ID | O |  | 6.2.3.3 | This IE shall not be used. *Global NG-RAN Node ID* IE shall replace this IE |
| >>Global NG-RAN Node ID | C-ifDCSetup |  | 6.2.3.2 | To be reported only by SN |
| >>Cell RNTI | O |  | 6.2.2.17 |  |
| *>gNB-DU / en-gNB-DU* |  |  |  | E2 node of type gNB-DU |
| >>gNB-CU UE F1AP ID | M |  | 6.2.3.21 |  |
| >>RAN UE ID | O |  | 6.2.3.25 |  |
| >>Cell RNTI | O |  | 6.2.2.17 |  |
| >*gNB-CU-UP / en-gNB-CU-UP* |  |  |  | E2 node of type gNB-CU-UP |
| >>gNB-CU-CP UE E1AP ID | M |  | 6.2.3.20 |  |
| >>RAN UE ID | O |  | 6.2.3.25 |  |
| *>ng-eNB* |  |  |  | E2 Node of type ng-eNB when connected to 5GC |
| >>AMF UE NGAP ID | M |  | 6.2.3.16 |  |
| >>GUAMI | M |  | 6.2.3.17 |  |
| >>ng-eNB-CU UE W1AP ID | C-ifCUDUseparated |  | 6.2.3.22 |  |
| >>M-NG-RAN node UE XnAP ID | C-ifDCSetup |  | 6.2.3.19 | To be reported by both MN and SN. |
| >>Global ng-eNB ID | O |  | 6.2.3.8 | This IE shall not be used. *Global NG-RAN Node ID* IE shall replace this IE |
| >>Global NG-RAN Node ID | C-ifDCSetup |  | 6.2.3.2 | To be reported only by SN |
| >>Cell RNTI | O |  | 6.2.2.17 |  |
| *>ng-eNB-DU* |  |  |  | E2 node of type ng-eNB-DU |
| >> ng-eNB-CU UE W1AP ID | M |  | 6.2.3.22 |  |
| >>Cell RNTI | O |  | 6.2.2.17 |  |
| *>en-gNB* |  |  |  | E2 Node of type en-gNB when connected to EPC and EN-DC is established |
| >>MeNB UE X2AP ID | M |  | 6.2.3.23 |  |
| >>MeNB UE X2AP ID Extension | O |  | 6.2.3.24 |  |
| >>Global eNB ID | M |  | 6.2.3.9 |  |
| >>gNB-CU UE F1AP ID | C-ifCUDUseperated |  | 6.2.3.21 |  |
| >>gNB-CU-CP UE E1AP ID List | C-ifCPUPseparated |  |  |  |
| >>>gNB-CU UE E1AP ID Item |  | *1 .. <maxE1APId>* |  |  |
| >>>>gNB-CU-CP UE E1AP ID | M |  | 6.2.3.20 |  |
| >> RAN UE ID | O |  | 6.2.3.25 |  |
| >>Cell RNTI | O |  | 6.2.2.17 |  |
| *>eNB* |  |  |  | E2 Node of type eNB when connected to EPC. |
| >>MME UE S1AP ID | M |  | 6.2.3.26 |  |
| >>GUMMEI | M |  | 6.2.3.18 |  |
| >>MeNB UE X2AP ID | C-ifDCSetup |  | 6.2.3.23 | To be reported by MeNB and SeNB. |
| >>MeNB UE X2AP ID Extension | C-ifDCSetup |  | 6.2.3.24 | To be reported by MeNB and SeNB. |
| >>Global eNB ID | C-ifDCSetup |  | 6.2.3.9 | To be reported only by SeNB. |
| >>Cell RNTI | O |  | 6.2.2.17 |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| *maxF1APId* | Maximum number of F1AP UEID for a NR-NR DC is 4 |
| *maxE1APId* | Maximum number of E1AP UEID for UE connected with different CU-UP is 65535 |

|  |  |
| --- | --- |
| Condition | Explanation |
| ifDCSetup | This IE shall be present in messages from E2 Node to NearRT-RIC if DC is established, whereas from NearRT-RIC to E2 Node messages, this IE may not be included |
| ifCUDUseparated | This IE shall be present in messages from E2 Node to NearRT-RIC for a CU-DU separated ng-eNB or (en-)gNB, whereas from NearRT-RIC to E2 Node messages, this IE may not be included. |
| ifCPUPseparated | This IE shall be present in messages from E2 Node to NearRT-RIC for a CP-UP separated (en-)gNB, whereas from NearRT-RIC to E2 Node messages, this IE may not be included. |

#### 6.2.2.7 Group ID

This IE defines a generic "Group ID" suitable for both EPC and 5GC networks.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| CHOICE *Core type* | M |  |  |  |
| *>5GC* |  |  |  |  |
| >>IRFSP | M |  | 6.2.3.27 |  |
| *>EPC* |  |  |  |  |
| >>SPID | M |  | 6.2.3.28 |  |

#### 6.2.2.8 Core CP ID

This IE defines a generic "Core CP ID" suitable for both EPC and 5GC networks.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| CHOICE *Core type* | M |  |  |  |
| *>5GC* |  |  |  |  |
| >>GUAMI | M |  | 6.2.3.17 |  |
| *>EPC* |  |  |  |  |
| >>GUMMEI | M |  | 6.2.3.18 |  |

#### 6.2.2.9 QoS ID

This IE defines a generic "QoS ID" suitable for both EPC and 5GC networks.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| CHOICE *Core type* | M |  |  |  |
| *>5GC* |  |  |  |  |
| >>5QI | M |  | 6.2.3.13 |  |
| *>EPC* |  |  |  |  |
| >>QCI | M |  | 6.2.3.14 |  |

#### 6.2.2.10 Network Interface Type

This IE defines the type of a standardized Network Interface.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Interface Type | M |  | ENUMERATED (NG, Xn, F1, E1, S1, X2, W1, …) | NG refers to NG interface [6]  Xn refers to Xn interface [7]  F1 refers to F1 interface [8]  E1 refers to E1 interface [9]  S1 refers to S1 interface [10]  X2 refers to X2 interface [11]  W1 refers to W1 interface [12] |

#### 6.2.2.11 Network Interface Identifier

This IE defines the identifier of the network node terminating a specific network interface.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **CHOICE** *Interface Identifier* | M |  |  |  |
| *>NG* |  |  |  | For interface type NG [6] |
| >>GUAMI | M |  | 6.2.3.17 |  |
| *>Xn* |  |  |  | For interface type Xn [7] |
| >>Global NG-RAN Node ID | M |  | 6.2.3.2 |  |
| *>F1* |  |  |  | For interface type F1 [8] |
| >>Global gNB ID | M |  | 6.2.3.2 |  |
| >>gNB-DU ID | M |  | 6.2.3.6 |  |
| *>E1* |  |  |  | For interface type E1 [9] |
| >>Global gNB ID | M |  | 6.2.3.2 |  |
| >>gNB-CU-UP ID | M |  | 6.2.3.5 |  |
| *>S1* |  |  |  | For interface type S1 [10] |
| >>GUMMEI | M |  | 6.2.3.18 |  |
| *>X2* |  |  |  | For interface type X2 [11] |
| >>**CHOICE** *Node Type* | M |  |  |  |
| >>>Global eNB ID |  |  | 6.2.3.9 | For eNB |
| >>>Global en-gNB ID |  |  | 6.2.3.4 | For en-gNB |
| *>W1* |  |  |  | For interface type W1 [12] |
| >>Global ng-eNB ID | M |  | 6.2.3.8 |  |
| >>ng-eNB-DU ID | M |  | 6.2.3.10 |  |

#### 6.2.2.12 Network Interface Message ID

This IE defines the identifier for a specific message of a given Network Interface.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Interface Procedure ID | M |  | INTEGER | Elementary Procedure Code |
| Message Type | M |  | ENUMERATED (InitiatingMessage, SuccessfulOutcome, UnsuccessfulOutcome, …) |  |

#### 6.2.2.13 RRC Message ID

This IE defines the identifier for a specific RRC message defined in either TS 36.331 [14] or TS 38.331 [15].

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **CHOICE** *RRC Type* | M |  |  |  |
| *>LTE* |  |  |  |  |
| >>LTE RRC Class | M |  | ENUMERATED (BCCH-BCH, BCCH-BCH-MBMS, BCCH-DL-SCH, BCCH-DL-SCH-BR, BCCH-DL-SCH-MBMS, MCCH, PCCH, DL-CCCH, DL-DCCH, UL-CCCH, UL-DCCH, SC-MCCH, …) | Refers to RRC message class defined in TS 36.331 [14] clause 6.2.1. |
| *>NR* |  |  |  |  |
| >>NR RRC Class | M |  | ENUMERATED (BCCH-BCH, BCCH-DL-SCH, DL-CCCH, DL-DCCH, PCCH, UL-CCCH, UL-CCCH1, UL-DCCH, …) | Refers to RRC message class defined in TS 38.331 [15] clause 6.2.1. |
| RRC Message ID | M |  | INTEGER | Number starts from 0 from the first entry of a given RRC message class defined in TS 36.331 [14] or TS 38.331 [15]. |

#### 6.2.2.14 Serving Cell PCI

This IE is used to identify the serving cell PCI in an E2 Node. The IE is derived from TS 38.473 [8] clause 9.3.1.10 and TS 36.423 [11] clause 9.2.8.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **CHOICE** *RAT type* | M |  |  |  |
| *>NR* |  |  |  |  |
| >>NR PCI | M |  | 6.2.3.29 |  |
| *>E-UTRA* |  |  |  |  |
| >>E-UTRA PCI | M |  | 6.2.3.32 |  |

#### 6.2.2.15 Serving Cell ARFCN

This IE is used to identify the serving cell ARFCN in an E2 Node. The IE is derived from TS 38.473 [8] clause 9.3.1.17 and TS 36.423 [11] clause 9.2.26.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| **CHOICE** *RAT type* | M |  |  |  |
| *>NR* |  |  |  |  |
| >>NR ARFCN | M |  | 6.2.3.30 |  |
| *>E-UTRA* |  |  |  |  |
| >>EARFCN | M |  | 6.2.3.33 |  |

#### 6.2.2.16 Beam ID

This IE is used to identify the generic "Beam ID" suitable for NR radio access technology (RAT).

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| CHOICE *RAT* | M |  |  |  |
| *>NR* |  |  |  |  |
| >>NR SSB-index | M |  | 6.2.3.36 | SSB-Index is used in NR as the Beam identifier |

#### 6.2.2.17 Cell RNTI

This represents a temporary UE Identifier in a cell in a Radio Network.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| C-RNTI | M |  | 6.2.3.37 |  |
| Cell Global ID | M |  | 6.2.2.5 | Identifies the cell where the C-RNTI is generated |

#### 6.2.2.18 Partial UE ID

This IE contains the UE ID data structure to be used for communication from Near-RT RIC to E2 Node.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| AMF UE NGAP ID | O |  | 6.2.3.16 |  |
| GUAMI | O |  | 6.2.3.17 |  |
| gNB-CU UE F1AP ID | O |  | 6.2.3.21 |  |
| gNB-CU-CP UE E1AP ID | O |  | 6.2.3.20 |  |
| RAN UE ID | O |  | 6.2.3.25 |  |
| M-NG-RAN node UE XnAP ID | O |  | 6.2.3.19 |  |
| Global NG-RAN Node ID | O |  | 6.2.3.2 |  |
| Cell RNTI | O |  | 6.2.2.17 |  |
| ng-eNB-CU UE W1AP ID | O |  | 6.2.3.22 |  |
| MeNB UE X2AP ID | O |  | 6.2.3.23 |  |
| MeNB UE X2AP ID Extension | O |  | 6.2.3.24 |  |
| Global eNB ID | O |  | 6.2.3.9 |  |
| MME UE S1AP ID | O |  | 6.2.3.26 |  |
| GUMMEI | O |  | 6.2.3.18 |  |

### 6.2.3 3GPP derived IEs

#### 6.2.3.1 PLMN Identity

This IE indicates the PLMN Identity.

Derived from 3GPP TS 38.413 [6] clause 9.3.3.5.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| PLMN Identity | M |  | OCTET STRING (SIZE(3)) | Defined in TS 38.413 [6] clause 9.3.3.5. |

#### 6.2.3.2 Global NG-RAN Node ID

This IE is used to globally identify an NG-RAN node of gNB and ng-eNB cases only.

Derived from 3GPP TS 38.423 [7] clause 9.2.2.3.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| CHOICE *NG-RAN node* | M |  |  |  |
| *>gNB* |  |  |  |  |
| >>Global gNB ID | M |  | 6.2.3.3 |  |
| >*ng-eNB* |  |  |  |  |
| >>Global ng-eNB ID | M |  | 6.2.3.8 |  |

#### 6.2.3.3 Global gNB ID

This IE is used to globally identify a gNB.

Derived from TS 38.413 [6] clause 9.3.1.6.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| PLMN Identity | M |  | 6.2.3.1 |  |
| CHOICE *gNB ID* | M |  |  |  |
| *>gNB ID* |  |  |  |  |
| >>gNB ID | M |  | BIT STRING (SIZE(22..32)) | Defined in TS 38.413 [6] clause 9.3.1.6. |

#### 6.2.3.4 Global en-gNB ID

This IE is used to globally identify an en-gNB.

Derived from TS 36.423 [11] clause 9.2.112.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| PLMN Identity | M |  | 6.2.3.1 |  |
| CHOICE *en-gNB ID* | M |  |  |  |
| *>en-gNB ID* |  |  |  |  |
| >>en-gNB ID | M |  | BIT STRING (SIZE(22..32)) | Defined in TS 36.423 [11] clause 9.2.112. |

#### 6.2.3.5 gNB-CU-UP ID

This IE uniquely identifies the gNB-CU-UP at least within a gNB-CU-CP.

Derived from TS 37.483 [9] clause 9.3.1.15.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| gNB-CU-UP ID | M |  | INTEGER (0 .. 236-1) | Defined in TS 37.483 [9] clause 9.3.1.15. |

#### 6.2.3.6 gNB-DU ID

This IE uniquely identifies the gNB-DU at least within a gNB-CU.

Derived from TS 38.473 [8] clause 9.3.1.9.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| gNB-DU ID | M |  | INTEGER (0 .. 236-1) | Defined in TS 38.473 [8] clause 9.3.1.9. |

#### 6.2.3.7 NR CGI

This IE is used to globally identify an NR cell.

Derived from TS 38.413 [6] clause 9.3.1.7.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| PLMN Identity | M |  | 6.2.3.1 |  |
| NR Cell Identity | M |  | BIT STRING (SIZE(36)) | Defined in TS 38.413 [6] clause 9.3.1.7. |

#### 6.2.3.8 Global ng-eNB ID

This IE is used to globally identify an ng-eNB.

Derived from TS 38.413 [6] clause 9.3.1.8.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| PLMN Identity | M |  | 6.2.3.1 |  |
| CHOICE *ng-eNB ID* | M |  |  |  |
| *>Macro ng-eNB ID* |  |  |  |  |
| >>Macro ng-eNB ID | M |  | BIT STRING (SIZE(20)) | Defined in TS 38.413 [6] clause 9.3.1.8. |
| *>Short Macro ng-eNB ID* |  |  |  |  |
| >>Short Macro ng-eNB ID | M |  | BIT STRING (SIZE(18)) | Defined in TS 38.413 [6] clause 9.3.1.8. |
| *>Long Macro ng-eNB ID* |  |  |  |  |
| >>Long Macro ng-eNB ID | M |  | BIT STRING (SIZE(21)) | Defined in TS 38.413 [6] clause 9.3.1.8. |

#### 6.2.3.9 Global eNB ID

This IE is used to globally identify an eNB.

Derived from TS 36.413 [10] clause 9.2.1.37.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| PLMN Identity | M |  | 6.2.3.1 |  |
| CHOICE *eNB ID* | M |  |  |  |
| *>Macro eNB ID* |  |  |  |  |
| >>Macro eNB ID | M |  | BIT STRING (SIZE(20)) | Defined in TS 36.413 [10] clause 9.2.1.37 |
| *>Home eNB ID* |  |  |  |  |
| >>Home eNB ID | M |  | BIT STRING (SIZE(28)) | Defined in TS 36.413 [10] clause 9.2.1.37. |
| *>Short Macro eNB ID* |  |  |  |  |
| >> Short Macro eNB ID | M |  | BIT STRING (SIZE(18)) | Defined in TS 36.413 [10] clause 9.2.1.37. |
| *>Long Macro eNB ID* |  |  |  |  |
| >> Long Macro eNB ID | M |  | BIT STRING (SIZE(21)) | Defined in TS 36.413 [10] clause 9.2.1.37. |

#### 6.2.3.10 ng-eNB-DU ID

This IE uniquely identifies the ng-eNB-DU at least within an ng-eNB-CU.

Derived from TS 37.473 [12] clause 9.3.1.9.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| ng-eNB-DU ID | M |  | INTEGER (0 .. 236-1) | Defined in TS 37.473 [12] clause 9.3.1.9. |

#### 6.2.3.11 E-UTRA CGI

This IE is used to globally identify an E-UTRA cell.

Derived from TS 38.413 [6] clause 9.3.1.9.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| PLMN Identity | M |  | 6.2.3.1 |  |
| E-UTRA Cell Identity | M |  | BIT STRING (SIZE(28)) | Defined in TS 38.413 [6] clause 9.3.1.9. |

#### 6.2.3.12 S-NSSAI

This IE is used to indicate the S-NSSAI.

Derived from TS 38.413 [6] clause 9.3.1.24.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| SST | M |  | OCTET STRING (SIZE(1)) | Defined in TS 38.413 [6] clause 9.3.1.24. |
| SD | O |  | OCTET STRING (SIZE(3)) | Defined in TS 38.413 [6] clause 9.3.1.24. |

#### 6.2.3.13 5QI

This IE is used to indicate 5QI value.

Derived from TS 38.413 [6] clause 9.3.1.28.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| 5QI | M |  | INTEGER (0..255, ...) | Defined in TS 38.413 [6] clause 9.3.1.28. |

#### 6.2.3.14 QCI

This IE is used to indicate QCI value.

Derived from TS 36.413 [10] clause 9.2.1.15.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| QCI | M |  | INTEGER (0..255) | Defined in TS 36.413 [10] clause 9.2.1.15. |

#### 6.2.3.15 QoS Flow Identifier (QFI)

This IE identifies a QoS flow within a PDU Session.

Derived from TS 38.413 [6] clause 9.3.1.51.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| QoS Flow Identifier | M |  | INTEGER (0..63, …) | Defined in TS 38.413 [6] clause 9.3.1.51. |

#### 6.2.3.16 AMF UE NGAP ID

This IE uniquely identifies a UE over the NG interface within a NG-RAN node.

Derived from 3GPP TS 38.413 [6] clause 9.3.3.1.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| AMF UE NGAP ID | M |  | INTEGER (0..240 -1) | Defined in TS 38.413 [6] clause 9.3.3.1. |

#### 6.2.3.17 GUAMI

This IE indicates the AMF identity.

Derived from 38.413 [6] clause 9.3.3.3.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| PLMN Identity | M |  | 6.2.3.1 |  |
| AMF Region ID | M |  | BIT STRING (SIZE(8)) |  |
| AMF Set ID | M |  | BIT STRING (SIZE(10)) | Defined in TS 38.413 [6] clause 9.3.3.12. |
| AMF Pointer | M |  | BIT STRING (SIZE(6)) | Defined in TS 38.413 [6] clause 9.3.3.19. |

#### 6.2.3.18 GUMMEI

This IE indicates the globally unique MME identity.

Derived from TS 36.413 [10] clause 9.2.3.9.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| PLMN Identity | M |  | 6.2.3.1 |  |
| MME Group ID | M |  | OCTET STRING (SIZE(2)) |  |
| MME code | M |  | OCTET STRING (SIZE (1)) | Defined in TS 36.413 [10] clause 9.2.3.12. |

#### 6.2.3.19 NG-RAN Node UE XnAP ID

This IE uniquely identifies a UE over the Xn interface within a NG-RAN node.

Derived from TS 38.423 [7] clause 9.2.3.16.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| NG-RAN node UE XnAP ID | M |  | INTEGER (0 .. 232 -1) | Defined in TS 38.423 [7] clause 9.2.3.16. |

#### 6.2.3.20 gNB-CU-CP UE E1AP ID

This IE uniquely identifies a UE over the E1 interface within a gNB-CU-CP.

Derived from TS 37.483 [9] clause 9.3.1.4.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| gNB-CU-CP UE E1AP ID | M |  | INTEGER (0 .. 232 -1) | Defined in TS 37.483 [9] clause 9.3.1.4. |

#### 6.2.3.21 gNB-CU UE F1AP ID

This IE uniquely identifies a UE over the F1 interface within a gNB-CU.

Derived from TS 38.473 [8] clause 9.3.1.4.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| gNB-CU UE F1AP ID | M |  | INTEGER (0 .. 232 -1) | Defined in TS 38.473 [8] clause 9.3.1.4. |

#### 6.2.3.22 ng-eNB-CU UE W1AP ID

This IE uniquely identifies a UE over the W1 interface within an ng-eNB-CU.

Derived from TS 37.473 [12] clause 9.3.1.4.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| ng-eNB-CU UE W1AP ID | M |  | INTEGER (0 .. 232 -1) | Defined in TS 37.473 [12] clause 9.3.1.4. |

#### 6.2.3.23 eNB UE X2AP ID

This IE, combined with the eNB UE X2AP ID Extension when present regardless its value, uniquely identifies a UE over the X2 interface within an eNB.

Derived from TS 36.423 [11] clause 9.2.24.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| eNB UE X2AP ID | M |  | INTEGER (0..4095) | Defined in TS 36.423 [11] clause 9.2.24. |

#### 6.2.3.24 eNB UE X2AP ID Extension

This IE, combined with the eNB UE X2AP ID uniquely identifies a UE over the X2 interface within an eNB. If the setup of an UE associated signalling connection was initiated including the eNB UE X2AP ID Extension, the eNB UE X2AP ID Extension shall be used by both peers for the life-time of the respective UE-associated signalling connection.

Derived from TS 36.423 [11] clause 9.2.86.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| eNB UE X2AP ID Extension | M |  | INTEGER (0..4095, …) | Defined in TS 36.423 [11] clause 9.2.86. |

#### 6.2.3.25 RAN UE ID

This UE Identifier identifies an UE over E1 and F1 interface within a gNB.

Derived from TS 38.473 [8] clause 9.2.2.1.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| RAN UE ID | O |  | OCTET STRING (SIZE (8)) | Defined in TS 38.473 [8] clause 9.2.2.1 |

#### 6.2.3.26 MME UE S1AP ID

This IE uniquely identifies a UE over the S1 interface within a MME.

Derived from TS 36.413 [10] clause 9.2.3.3.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| MME UE S1AP ID | M |  | INTEGER (0 .. 232 -1) | Defined in TS 36.413 [10] clause 9.2.3.3. |

#### 6.2.3.27 Index to RAT/Frequency Selection Priority (IRFSP)

This IE is used to define local configuration for RRM strategies such as camp priorities in Idle mode and control of inter-RAT/inter-frequency handover in Active mode.

Derived from TS 38.413 [6] clause 9.3.1.61.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Index to RAT/Frequency Selection Priority | M |  | INTEGER (1..256, …) | Defined in TS 38.413 [6] clause 9.3.1.61. |

#### 6.2.3.28 Subscriber Profile ID for RAT/Frequency priority (SPID)

This IE is used to define camp priorities in Idle mode and to control inter-RAT/inter-frequency handover in Active mode.

Derived from TS 36.413 [10] clause 9.2.1.39.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| Subscriber Profile ID for RAT/Frequency Priority | M |  | INTEGER (1..256) | Defined in TS 36.413 [10] clause 9.2.1.39. |

#### 6.2.3.29 NR PCI

This IE is used to identify an NR cell PCI.

Derived from TS 38.473 [8] clause 9.3.1.10.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| NR PCI | M |  | INTEGER  (0.. 1007) | Derived from TS 38.473 [8] clause 9.3.1.10. |

#### 6.2.3.30 NR ARFCN

This IE is used to identify an NR ARFCN.

Derived from TS 38.473 [8] clause 9.3.1.17.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| NR ARFCN | M |  | INTEGER (0..maxNRARFCN) | Derived from TS 38.473 [8] clause 9.3.1.17. |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxNRARFCN | Maximum value of NR ARFCNs. Value is 3279165. |

#### 6.2.3.31 5GS TAC

This IE is used to identify 5GS Tracking Area Code.

Defined in TS 38.473 [8] clause 9.3.1.29.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| 5GS TAC | M |  | OCTET STRING (SIZE (3)) | Defined in TS 38.473 [8] clause 9.3.1.29. |

#### 6.2.3.32 E-UTRA PCI

This IE is used to identify an E-UTRA cell PCI.

Derived from TS 36.423 [11] clause 9.2.8.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| E-UTRA PCI | M |  | INTEGER  (0.. 503, …) | Derived from TS 36.423 [11] clause 9.2.8. |

#### 6.2.3.33 E-UTRA ARFCN

This IE is used to identify an E-UTRA Frequency Info.

Defined in TS 36.423 [11] clause 9.2.26.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| EARFCN | M |  | INTEGER (0.. maxEARFCN) | Defined in TS 36.423 [11] clause 9.2.26. |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxEARFCN | Maximum value of EARFCNs. Value is 65535. |

#### 6.2.3.34 E-UTRA TAC

This IE is used to identify an E-UTRA Tracking Area Code.

Derived from TS 36.423 [11] clause 9.2.8.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| E-UTRA TAC | M |  | OCTET STRING (SIZE(2)) | Derived from TS 36.423 [11] clause 9.2.8. |

#### 6.2.3.35 NR Frequency Info

This IE is used to define the carrier frequency and bands used in a cell.

Derived from TS 38.473 [8] clause 9.3.1.17.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE Type and Reference | Semantics Description |
| NR ARFCN | M |  | 6.2.3.30 |  |
| NR Frequency Band List |  | *1* |  |  |
| >NR Frequency Band Item |  | *1..<maxnoofNRCellBands>* |  |  |
| >>NR Frequency Band | M |  | INTEGER (1.. 1024, ...) | Defined in TS 38.473 [8] clause 9.3.1.17 |
| >>Supported SUL band List |  | *0..<maxnoofNRCellBands>* |  |  |
| >>>Supported SUL band Item | M |  | INTEGER (1.. 1024, ...) | Defined in TS 38.473 [8] clause 9.3.1.17 |
| NRFrequency Shift 7p5khz | O |  | ENUMERATED (false, true, ...) | Defined in TS 38.473 [8] clause 9.3.1.17 |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofNRCellBands | Maximum no. of frequency bands supported for a NR cell. Value is 32. |

#### 6.2.3.36 NR SSB-Index

This IE is used to identify the NR SSB-Index.

Derived from TS 38.331 [15] clause 6.3.2.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| SSB-Index | M |  | INTEGER  (0.. maxNrofSSBs-1) | Derived from TS 38.331 [15] clause 6.3.2. |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxNrofSSBs-1 | Maximum number of SSB resources in a resource set minus 1. Value is 63. |

#### 6.2.3.37 C-RNTI

This represents a temporary UE Identifier in a cell in a Radio Network.

Derived from TS 38.331 [15] clause 6.3.2.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| C-RNTI | M |  | INTEGER (0..65535) | Defined in TS 38.331 [15] clause 6.3.2. |

## 6.3 Information Element Abstract Syntax (with ASN.1)

### 6.3.1 General

E2SM ASN.1 definition conforms to ITU-T Rec. X.680 [16] and ITU-T Rec. X.681 [17].

Sub clause 6.3.2 presents the Abstract Syntax of the common E2SM information elements that may be used with RAN Function specific E2AP [3] Information Elements when encoded using ASN.1. In case there is contradiction between the ASN.1 definition in this sub clause and the tabular format in sub clause 6.2, the ASN.1 shall take precedence, except for the definition of conditions for the presence of conditional elements, in which the tabular format shall take precedence.

### 6.3.2 Information Element definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- E2SM

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E2SM-COMMON-IEs {

iso(1) identified-organization(3) dod(6) internet(1) private(4) enterprise(1) oran(53148) e2(1) version1 (1) e2sm(2) e2sm-COMMON-IEs (0)}

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- --------------------------------------------------

#### -- Constants

-- --------------------------------------------------

maxE1APid INTEGER ::= 65535

maxF1APid INTEGER ::= 4

-- IEs derived from 3GPP 36.423 (X2AP)

maxEARFCN INTEGER ::= 65535

-- IEs derived from 3GPP 38.473 (F1AP)

maxNRARFCN INTEGER ::= 3279165

maxnoofNrCellBands INTEGER ::= 32

-- IEs derived from 3GPP 38.331 (NR RRC)

maxNrofSSBs-1 INTEGER ::= 63

-- --------------------------------------------------

#### -- E2SM Commmon IEs

-- --------------------------------------------------

Beam-ID ::= CHOICE {

nR-Beam-ID NR-SSB-Index,

...

}

Cell-RNTI ::= SEQUENCE {

c-RNTI RNTI-Value,

cell-Global-ID CGI,

...

}

CGI ::= CHOICE {

nR-CGI NR-CGI,

eUTRA-CGI EUTRA-CGI,

...

}

CoreCPID ::= CHOICE {

fiveGC GUAMI,

ePC GUMMEI,

...

}

InterfaceIdentifier ::= CHOICE {

nG InterfaceID-NG,

xN InterfaceID-Xn,

f1 InterfaceID-F1,

e1 InterfaceID-E1,

s1 InterfaceID-S1,

x2 InterfaceID-X2,

w1 InterfaceID-W1,

...

}

InterfaceID-NG ::= SEQUENCE {

guami GUAMI,

...

}

InterfaceID-Xn ::= SEQUENCE {

global-NG-RAN-ID GlobalNGRANNodeID,

...

}

InterfaceID-F1 ::= SEQUENCE {

globalGNB-ID GlobalGNB-ID,

gNB-DU-ID GNB-DU-ID,

...

}

InterfaceID-E1 ::= SEQUENCE {

globalGNB-ID GlobalGNB-ID,

gNB-CU-UP-ID GNB-CU-UP-ID,

...

}

InterfaceID-S1 ::= SEQUENCE {

gUMMEI GUMMEI,

...

}

InterfaceID-X2 ::= SEQUENCE {

nodeType CHOICE {

global-eNB-ID GlobalENB-ID,

global-en-gNB-ID GlobalenGNB-ID,

...

},

...

}

InterfaceID-W1 ::= SEQUENCE {

global-ng-eNB-ID GlobalNgENB-ID,

ng-eNB-DU-ID NGENB-DU-ID,

...

}

Interface-MessageID ::= SEQUENCE {

interfaceProcedureID INTEGER,

messageType ENUMERATED {initiatingMessage, successfulOutcome, unsuccessfulOutcome, ...},

...

}

InterfaceType ::= ENUMERATED {nG, xn, f1, e1, s1, x2, w1, ...}

GroupID ::= CHOICE {

fiveGC FiveQI,

ePC QCI,

...

}

PartialUEID ::= SEQUENCE {

amf-UE-NGAP-ID AMF-UE-NGAP-ID OPTIONAL,

guami GUAMI OPTIONAL,

gNB-CU-UE-F1AP-ID GNB-CU-UE-F1AP-ID OPTIONAL,

gNB-CU-CP-UE-E1AP-ID GNB-CU-CP-UE-E1AP-ID OPTIONAL,

ran-UEID RANUEID OPTIONAL,

m-NG-RAN-UE-XnAP-ID NG-RANnodeUEXnAPID OPTIONAL,

globalNG-RANNode-ID GlobalNGRANNodeID OPTIONAL,

cell-RNTI Cell-RNTI OPTIONAL,

ng-eNB-CU-UE-W1AP-ID NGENB-CU-UE-W1AP-ID OPTIONAL,

m-eNB-UE-X2AP-ID ENB-UE-X2AP-ID OPTIONAL,

m-eNB-UE-X2AP-ID-Extension ENB-UE-X2AP-ID-Extension OPTIONAL,

globalENB-ID GlobalENB-ID OPTIONAL,

mME-UE-S1AP-ID MME-UE-S1AP-ID OPTIONAL,

gUMMEI GUMMEI OPTIONAL,

...

}

QoSID ::= CHOICE {

fiveGC FiveQI,

ePC QCI,

...

}

RANfunction-Name ::= SEQUENCE{

ranFunction-ShortName PrintableString(SIZE(1..150,...)),

ranFunction-E2SM-OID PrintableString(SIZE(1..1000,...)),

ranFunction-Description PrintableString(SIZE(1..150,...)),

ranFunction-Instance INTEGER OPTIONAL,

...

}

RIC-Format-Type ::= INTEGER

RIC-Style-Type ::= INTEGER

RIC-Style-Name ::= PrintableString(SIZE(1..150,...))

RRC-MessageID ::= SEQUENCE {

rrcType CHOICE {

lTE RRCclass-LTE,

nR RRCclass-NR,

...

},

messageID INTEGER,

...

}

RRCclass-LTE ::= ENUMERATED {bCCH-BCH, bCCH-BCH-MBMS, bCCH-DL-SCH, bCCH-DL-SCH-BR, bCCH-DL-SCH-MBMS, mCCH, pCCH, dL-CCCH, dL-DCCH, uL-CCCH, uL-DCCH, sC-MCCH, ...}

RRCclass-NR ::= ENUMERATED {bCCH-BCH, bCCH-DL-SCH, dL-CCCH, dL-DCCH, pCCH, uL-CCCH, uL-CCCH1, uL-DCCH, ...}

ServingCell-ARFCN ::= CHOICE {

nR NR-ARFCN,

eUTRA E-UTRA-ARFCN,

...

}

ServingCell-PCI ::= CHOICE {

nR NR-PCI,

eUTRA E-UTRA-PCI,

...

}

UEID ::= CHOICE{

gNB-UEID UEID-GNB,

gNB-DU-UEID UEID-GNB-DU,

gNB-CU-UP-UEID UEID-GNB-CU-UP,

ng-eNB-UEID UEID-NG-ENB,

ng-eNB-DU-UEID UEID-NG-ENB-DU,

en-gNB-UEID UEID-EN-GNB,

eNB-UEID UEID-ENB,

...

}

UEID-GNB ::= SEQUENCE{

amf-UE-NGAP-ID AMF-UE-NGAP-ID,

guami GUAMI,

gNB-CU-UE-F1AP-ID-List UEID-GNB-CU-F1AP-ID-List OPTIONAL,

-- C-ifCUDUseparated: This IE shall be present in messages from E2 Node to NearRT-RIC for a CU-DU separated gNB, whereas from NearRT-RIC to E2 Node messages, this IE may not be included. More than 1 F1AP ID shall be reported by E2 Node only when NR-DC is established.

gNB-CU-CP-UE-E1AP-ID-List UEID-GNB-CU-CP-E1AP-ID-List OPTIONAL,

-- C-ifCPUPseparated: This IE shall be present in messages from E2 Node to NearRT-RIC for a CP-UP separated gNB, whereas from NearRT-RIC to E2 Node messages, this IE may not be included.

ran-UEID RANUEID OPTIONAL,

m-NG-RAN-UE-XnAP-ID NG-RANnodeUEXnAPID OPTIONAL,

-- C-ifDCSetup: This IE shall be present in messages from E2 Node to NearRT-RIC if DC is established, whereas from NearRT-RIC to E2 Node messages, this IE may not be included. To be reported by both MN and SN.

globalGNB-ID GlobalGNB-ID OPTIONAL,

-- This IE shall not be used. This IE is replaced with globalNG-RANNode-ID.

...,

globalNG-RANNode-ID GlobalNGRANNodeID OPTIONAL,

-- C-ifDCSetup: This IE shall be present in messages from E2 Node to NearRT-RIC if DC is established, whereas from NearRT-RIC to E2 Node messages, this IE may not be included. To be reported only by SN.

cell-RNTI Cell-RNTI OPTIONAL

}

UEID-GNB-CU-CP-E1AP-ID-List ::= SEQUENCE (SIZE(1..maxE1APid)) OF UEID-GNB-CU-CP-E1AP-ID-Item

UEID-GNB-CU-CP-E1AP-ID-Item ::= SEQUENCE{

gNB-CU-CP-UE-E1AP-ID GNB-CU-CP-UE-E1AP-ID,

...

}

UEID-GNB-CU-F1AP-ID-List ::= SEQUENCE (SIZE(1..maxF1APid)) OF UEID-GNB-CU-CP-F1AP-ID-Item

UEID-GNB-CU-CP-F1AP-ID-Item ::= SEQUENCE{

gNB-CU-UE-F1AP-ID GNB-CU-UE-F1AP-ID,

...

}

UEID-GNB-DU ::= SEQUENCE{

gNB-CU-UE-F1AP-ID GNB-CU-UE-F1AP-ID,

ran-UEID RANUEID OPTIONAL,

...,

cell-RNTI Cell-RNTI OPTIONAL

}

UEID-GNB-CU-UP ::= SEQUENCE{

gNB-CU-CP-UE-E1AP-ID GNB-CU-CP-UE-E1AP-ID,

ran-UEID RANUEID OPTIONAL,

...

}

UEID-NG-ENB ::= SEQUENCE{

amf-UE-NGAP-ID AMF-UE-NGAP-ID,

guami GUAMI,

ng-eNB-CU-UE-W1AP-ID NGENB-CU-UE-W1AP-ID OPTIONAL,

-- C-ifCUDUseperated: This IE shall be present in messages from E2 Node to NearRT-RIC for a CU-DU seperated ng-eNB, whereas from NearRT-RIC to E2 Node messages, this IE may not be included.

m-NG-RAN-UE-XnAP-ID NG-RANnodeUEXnAPID OPTIONAL,

-- C-ifDCSetup: This IE shall be present in messages from E2 Node to NearRT-RIC if DC is established, whereas from NearRT-RIC to E2 Node messages, this IE may not be included. To be reported by both MN and SN.

globalNgENB-ID GlobalNgENB-ID OPTIONAL,

-- This IE shall not be used. This IE is replaced with globalNG-RANNode-ID.

...,

globalNG-RANNode-ID GlobalNGRANNodeID OPTIONAL,

-- C-ifDCSetup: This IE shall be present in messages from E2 Node to NearRT-RIC if DC is established, whereas from NearRT-RIC to E2 Node messages, this IE may not be included. To be reported only by SN.

cell-RNTI Cell-RNTI OPTIONAL

}

UEID-NG-ENB-DU ::= SEQUENCE{

ng-eNB-CU-UE-W1AP-ID NGENB-CU-UE-W1AP-ID,

...,

cell-RNTI Cell-RNTI OPTIONAL

}

UEID-EN-GNB ::= SEQUENCE{

m-eNB-UE-X2AP-ID ENB-UE-X2AP-ID,

m-eNB-UE-X2AP-ID-Extension ENB-UE-X2AP-ID-Extension OPTIONAL,

globalENB-ID GlobalENB-ID,

gNB-CU-UE-F1AP-ID GNB-CU-UE-F1AP-ID OPTIONAL,

-- C-ifCUDUseperated: This IE shall be present in messages from E2 Node to NearRT-RIC for a CU-DU seperated en-gNB, whereas from NearRT-RIC to E2 Node messages, this IE may not be included.

gNB-CU-CP-UE-E1AP-ID-List UEID-GNB-CU-CP-E1AP-ID-List OPTIONAL,

-- C-ifCPUPseparated: This IE shall be present in messages from E2 Node to NearRT-RIC for a CP-UP separated en-gNB, whereas from NearRT-RIC to E2 Node messages, this IE may not be included.

ran-UEID RANUEID OPTIONAL,

...,

cell-RNTI Cell-RNTI OPTIONAL

}

UEID-ENB ::= SEQUENCE{

mME-UE-S1AP-ID MME-UE-S1AP-ID,

gUMMEI GUMMEI,

m-eNB-UE-X2AP-ID ENB-UE-X2AP-ID OPTIONAL,

-- This IE shall be present in messages from E2 Node to NearRT-RIC if DC is established, whereas from NearRT-RIC to E2 Node messages, this IE may not be included. To be reported by MeNB and SeNB.

m-eNB-UE-X2AP-ID-Extension ENB-UE-X2AP-ID-Extension OPTIONAL,

globalENB-ID GlobalENB-ID OPTIONAL,

-- This IE shall be present in messages from E2 Node to NearRT-RIC if DC is established, whereas from NearRT-RIC to E2 Node messages, this IE may not be included. To be reported only by SeNB.

...,

cell-RNTI Cell-RNTI OPTIONAL

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

#### -- 3GPP derived IEs

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- NOTE:

-- - Extension fields removed and replaced with "..."

-- - IE names modified across all extracts to use "PLMNIdentity"

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- IEs derived from 3GPP 36.413 (S1AP)

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

ENB-ID ::= CHOICE {

macro-eNB-ID BIT STRING (SIZE (20)),

home-eNB-ID BIT STRING (SIZE (28)),

... ,

short-Macro-eNB-ID BIT STRING (SIZE(18)),

long-Macro-eNB-ID BIT STRING (SIZE(21))

}

GlobalENB-ID ::= SEQUENCE {

pLMNIdentity PLMNIdentity,

eNB-ID ENB-ID,

...

}

GUMMEI ::= SEQUENCE {

pLMN-Identity PLMNIdentity,

mME-Group-ID MME-Group-ID,

mME-Code MME-Code,

...

}

MME-Group-ID ::= OCTET STRING (SIZE (2))

MME-Code ::= OCTET STRING (SIZE (1))

MME-UE-S1AP-ID ::= INTEGER (0..4294967295)

QCI ::= INTEGER (0..255)

SubscriberProfileIDforRFP ::= INTEGER (1..256)

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- IEs derived from 3GPP 36.423 (X2AP)

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- Extension fields removed.

-- Note: to avoid duplicate names with NGAP, XnAP, etc.:

-- GNB-ID renamed ENGNB-ID,

-- GlobalGNB-ID renamed GlobalenGNB-ID,

-- UE-X2AP-ID renamed ENB-UE-X2AP-ID

-- UE-X2AP-ID-Extension renamed ENB-UE-X2AP-ID-Extension

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

EN-GNB-ID ::= CHOICE {

en-gNB-ID BIT STRING (SIZE (22..32)),

...

}

ENB-UE-X2AP-ID ::= INTEGER (0..4095)

ENB-UE-X2AP-ID-Extension ::= INTEGER (0..4095, ...)

E-UTRA-ARFCN ::= INTEGER (0..maxEARFCN)

E-UTRA-PCI ::= INTEGER (0..503, ...)

E-UTRA-TAC ::= OCTET STRING (SIZE(2))

GlobalenGNB-ID ::= SEQUENCE {

pLMN-Identity PLMNIdentity,

en-gNB-ID EN-GNB-ID,

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- IEs derived from 3GPP 37.473 (W1AP)

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NGENB-CU-UE-W1AP-ID ::= INTEGER (0..4294967295)

NGENB-DU-ID ::= INTEGER (0..68719476735)

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- IEs derived from 3GPP 38.331 (NR RRC)

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NR-SSB-Index ::= INTEGER (0..maxNrofSSBs-1)

RNTI-Value ::= INTEGER (0..65535)

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- IEs derived from 3GPP 38.413 (NGAP)

-- Extension fields removed and replaced with ...

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

AMFPointer ::= BIT STRING (SIZE(6))

AMFRegionID ::= BIT STRING (SIZE(8))

AMFSetID ::= BIT STRING (SIZE(10))

AMF-UE-NGAP-ID ::= INTEGER (0..1099511627775)

EUTRACellIdentity ::= BIT STRING (SIZE(28))

EUTRA-CGI ::= SEQUENCE {

pLMNIdentity PLMNIdentity,

eUTRACellIdentity EUTRACellIdentity,

...

}

FiveQI ::= INTEGER (0..255, ...)

GlobalGNB-ID ::= SEQUENCE {

pLMNIdentity PLMNIdentity,

gNB-ID GNB-ID,

...

}

GlobalNgENB-ID ::= SEQUENCE {

pLMNIdentity PLMNIdentity,

ngENB-ID NgENB-ID,

...

}

GNB-ID ::= CHOICE {

gNB-ID BIT STRING (SIZE(22..32)),

...

}

GUAMI ::= SEQUENCE {

pLMNIdentity PLMNIdentity,

aMFRegionID AMFRegionID,

aMFSetID AMFSetID,

aMFPointer AMFPointer,

...

}

IndexToRFSP ::= INTEGER (1..256, ...)

NgENB-ID ::= CHOICE {

macroNgENB-ID BIT STRING (SIZE(20)),

shortMacroNgENB-ID BIT STRING (SIZE(18)),

longMacroNgENB-ID BIT STRING (SIZE(21)),

...

}

NRCellIdentity ::= BIT STRING (SIZE(36))

NR-CGI ::= SEQUENCE {

pLMNIdentity PLMNIdentity,

nRCellIdentity NRCellIdentity,

...

}

PLMNIdentity ::= OCTET STRING (SIZE(3))

QosFlowIdentifier ::= INTEGER (0..63, ...)

SD ::= OCTET STRING (SIZE(3))

S-NSSAI ::= SEQUENCE {

sST SST,

sD SD OPTIONAL,

...

}

SST ::= OCTET STRING (SIZE(1))

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- IEs derived from 3GPP 38.423 (XnAP)

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NG-RANnodeUEXnAPID ::= INTEGER (0.. 4294967295)

GlobalNGRANNodeID ::= CHOICE {

gNB GlobalGNB-ID,

ng-eNB GlobalNgENB-ID,

...

}

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- IEs derived from 3GPP 37.483 (E1AP)

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

GNB-CU-CP-UE-E1AP-ID ::= INTEGER (0..4294967295)

GNB-CU-UP-ID ::= INTEGER (0..68719476735)

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- IEs derived from 3GPP 38.473 (F1AP)

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

FiveGS-TAC ::= OCTET STRING (SIZE(3))

FreqBandNrItem ::= SEQUENCE {

freqBandIndicatorNr INTEGER (1..1024, ...),

...

}

GNB-CU-UE-F1AP-ID ::= INTEGER (0..4294967295)

GNB-DU-ID ::= INTEGER (0..68719476735)

NR-PCI ::= INTEGER (0..1007)

NR-ARFCN ::= SEQUENCE {

nRARFCN INTEGER (0..maxNRARFCN),

...

}

NRFrequencyBand-List ::= SEQUENCE (SIZE(1..maxnoofNrCellBands)) OF NRFrequencyBandItem

NRFrequencyBandItem ::= SEQUENCE {

freqBandIndicatorNr INTEGER (1..1024,...),

supportedSULBandList SupportedSULBandList,

...

}

NRFrequencyInfo ::= SEQUENCE {

nrARFCN NR-ARFCN,

frequencyBand-List NRFrequencyBand-List,

frequencyShift7p5khz NRFrequencyShift7p5khz OPTIONAL,

...

}

NRFrequencyShift7p5khz ::= ENUMERATED {false, true, ...}

RANUEID ::= OCTET STRING (SIZE (8))

SupportedSULBandList ::= SEQUENCE (SIZE(0..maxnoofNrCellBands)) OF SupportedSULFreqBandItem

SupportedSULFreqBandItem ::= SEQUENCE {

freqBandIndicatorNr INTEGER (1..1024,...),

...

}

END

-- ASN1STOP

### 6.3.3 Message transfer syntax

E2SM shall use the ASN.1 Basic Packed Encoding Rules (BASIC-PER) Aligned Variant as transfer syntax, as specified in ITU-T Rec. X.691 [7].

# Annex (informative): Change History

| Date | Revision | Description |
| --- | --- | --- |
|  |  |  |
| **2020.01.22** | **01.00** | **Specification renamed v.01.00.00 for approval** |
|  |  |  |
| 2020.07.09 | 01.00.01 | Inclusion of agreed CR “E2SM Change to Annex A layout” |
| 2020.07.10 | 01.00.02 | Clarification in table 7.8-2 within the embedded example document Reference corrected in table in 8.2.2.1 |
| **2020.07.15** | **01.01** | **Incremented version for Publication** |
|  |  |  |
| 2021.05.28 | v02.00.01 | Inclusion of CR agreed at WG3#99 < NOK.AO-2021.05.05-WG3-CR-0001-E2SM+common+IEs-v01 >. Endorsed as WG3#100 |
| 2021.07.07 | v02.00.02 | Adopted INT.AO-CR-0010. |
| **2021.08.10** | **02.00** | **TSC approved** |
|  |  |  |
| 2021.11.09 | V02.01.01 | Inclusion of CR agreed at WG3#117 <RSYS-2021.10.05-WG3-CR-0001-E2SM-Common-Correction for UEID and NRARFCN\_v0.5>  Alignment of copyright notice |
| 2021.11.22 | V02.01.02 | Corrections based on WG3 review comments during WG3 approval process |
| **2022.02.07** | **02.01** | **Version ready for Nov 21 train** |
|  |  |  |
| 2022.10.27 | V02.01.01 | Addition of CR:  < NOK-2022.09.01-WG3-CR-0003-E2SM-E1AP reference correction-v03> error in CR corrected (ref [9] should be 37.483) < NOK-2022.10.31-WG3-CR-0004-E2SM-E2SM-CCC table entry-v01 >  Aligned for specification to latest O-RAN template |
| 2022.11.10 | V02.01.02 | Addition of CR: <QCM.AO-2022.10.27-WG3-CR-0001-E2SM-RIC Query-v03> |
| 2022.11.16 | V02.01.03 | Changes reflecting remarks received during WG3 approval process  - Alignment to latest O-RAN template  - Added R003 to file name  - Updated copyright year  - Corrected error in CRs implemented in previous drafts |
| **2022.12.07** | **03.00** | **Version ready for Nov 22 train** |
|  |  |  |
| 2023.02.16 | V03.00.01 | CR <NOK-2023.02.08-WG3-CR-0006-E2SM-PAS step1-v02> approved Prague F2F 16/2/2023 |
| 2023.03.24 | V03.00.02 | Inclusion of corrections agreed during WG3 approval process as per <O-RAN.WG3.E2SM-R003-v03.00.01-ApprovalChanges-v2> |
| **2023.03.24** | **03.01** | **Version ready for March 23 train** |
|  |  |  |
| 2023.05.15 | V03.01.01 | CR <NOK-2023.01.23-WG3-CR-0005-E2SM-Beam-ID-v02> approved WG3#180  CR <NOK-2023.04.28-WG3-CR-0007-E2SM-Correction to clause 2.1-v01> approved WG3#183 |
| 2023.06.27 | V03.01.02 | CR <QCM-2023.04.17-WG3-CR-0002-E2SM-Addition of C-RNTI-v01> approved F2F Osaka  Editorial correction to ASN.1 variable name "nR-Beam-ID" (was "nR-Beam\_ID") |
| 2023.07.26 | V03.01.03 | Editorial corrections based on comments received during WG3 poll. |
| 2023.07.27 | V03.01.04 | Editorial changes to align to O-RAN TS template v01.01 |
| **2023.07.31** | **04.00** | **Version ready for July 23 train** |
|  |  |  |
| 2023.10.30 | 04.00.01 | CR < QCM-2023.10.19-WG3-CR-0003-E2SM-UEID Structure for RIC Query\_v0> approved WG3#202, 25/10/2023. Editorial correction to IE name in ASN.1 |
| 2023.11.15 | 04.00.02 | Editorial corrections implementing WG3 voting period feedback |
| 2023.11.21 | 04.00.03 | Restored full revision history into Annex: Change History and deletion of Annex: History | |
| **2023.11.21** | **05.00** | **Version ready for Nov. 23 train** |
|  |  |  |